|  |  |  |
| --- | --- | --- |
| A 1x3  2-8 ABC  Active | B 1x1  <=40 EEE  Reagent Corrosive | C 1x1  >=25 D  Buffer |
| D 2x3  2-8 ABC  Buffer | E 3x1  <=40 EEE  Active | F 2x1  <=40 D  Reagent Toxic |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |